HC11IDE and MOTOROLA EVBU
-------------------------

If you want to use the HC11IDE software together with the Motorola Universal 
Evaluation Board (M68HC11EVBU) you have to do the following modifications:

1. Connect a schottky type diode to U4 pin 16 (cathode) and RN1 pin 2 (anode).
Now the EVBU can be resetted by the PC software.

2. Replace the 'E9 MCU with a MC68HC11A1 or MC68HC811E2. The MC68HC11E9 MCU
is currently not supported by the HC11IDE software.

3. Connect the EVBU to the COM1 port of your PC via a 1:1 cable (do not use
a null modem cable).
