Hi, there,
in this package you find some update information about the article in
E l e k t o r  4/94. The usage of the minidebugger (MINIBUG) is possible,
although there is a more powerful tool available on the Motorola Mailbox called
PCBUG11.
PCBUG11 has better Debug functions like BREAKPOINT-SET, TRACE of SOFTWARE
        BLOCKFILL, LINE ASSEMBLER, DISASSEMBLER,
        ENABLE EEPROM for DOUNLOAD of ASSEMBLER output files (Files.S19)
        and PROGAM EEPROM MEMORY, or ERASE EEPROM COMMAND etc.
        CONTROL-Comands (e.g.'CONTROL BASE HEX' is ENABLE ADDRESS DATA input
        in HEX) etc.....
You need only ASMHC11 for using PCBUG11 in order to make ASSEMBLER FILES.
For creating  .BOO Files you can use ASSEMBLER options or make conversion
of ASSEMBLER output Files  .S19 -> .BOO with RECBOOT

Within this package you find the newest version of the HC11 freeware
assembler.

For Minibug.bat problems:
         Pleas change last line from KERMIT ( TERMINAL PROGAM ) to your
         Terminal Software. KERMIT is only for communication to HC11 used.

Some Literature helps:
   
   - Single- and Multiple-Chip Microcomputer Interfacing
     Autor: G.L. LIPOVSKI
     PRENTICE HALL Englewood Cliffs, N.J. 07632
     ISBN 0-13-810557-X  025 {PRENTICE-HALL ED .}
     ISBN 0-13-810573-1

     - Single- and Multiple-Chip Microcomputer Interfacing
       Laboratory Manual
     Autor: G.L. LIPOVSKI
     PRENTICE HALL Englewood Cliffs, N.J. 07632
     ISBN  0-13-811605-9


  - Steuer- und Regelungstechnik mit Single-Chip-Mikroprozessoren
    mit Softwarebeispiele Cross-Assembler Diskette und Leiterplatte
    von Rose, Michael
    1991 Huethig Buch Verlag GmbH, Heidelberg
    ISBN 3-7785-2063-6
